**COMPARATIVE STUDY OF UNBRACED, CROSSED AND DIAGONALLY BRACED FRAME OF MID RISE BUILDING TO BE CONSTRUCTED IN HILLY AREA**

**Harsh Joshi1 Prof. Dr. Savita Maru2**

1PG student at Department of civil engineering, Ujjain engineering college, Ujjain,M.P., India

2 Professor at Department of civil engineering Ujjain engineering college Ujjain Ujjain,M.P., India

**ABSTRACT**

Due to sloping land and high seismically active zones, designing and construction of multistory buildings in hilly regions is always a challenge for structural engineers. This review paper focuses to establish a review study on the Possible Types of building frame configuration in the hilly region and he behavior of Such building frames under seismic loading conditions, and (3) The recent research and developments to make such frames less vulnerable to earthquakes.

This paper concludes that the dynamics characteristics of such buildings are significantly different in both horizontal and vertical directions, resulting in the center of mass and center of stiffness having eccentricity at point of action and not vertically aligned for different floors. When such frames are subjected to lateral loads, due to eccentricity it generates torsion in the frame. Most of the studies agree that the buildings resting on slanting ground have higher displacement and base shear compared to buildings resting on plain ground and the shorter column attracts more forces and undergoes damage when subjected to earthquake. This paper conclude the computational experiment done on G+ 4 & G +7 building with different bracing patterns located in seismic zone V and in hilly area.

*Keywords: Building frame configuration, Seismic behavior, Dynamic characteristics, Response spectrum analysis, time history analysis.*

1. **INTRODUCTION**

The behavior of a building during an earthquake depends on various uncertainties. These uncertainties are due to various causes, the nature of the earthquake, the behavior of the components, and the method of analysis. Therefore, the response of the building depends on the movement of the ground and the editing of the individual responses of the structural and non-structural components in a fully stochastic framework. Past seismic experience has shown that many common buildings and typical construction methods lack basic resistance to seismic forces. This resistance can most often be achieved by the simple and inexpensive principles of good building practices. Adherence to these simple rules will not prevent all damage in moderate or large earthquakes, but life threatening collapses should be prevented, and damage limited to repairable proportions. These principles fall into several broad categories

Planning and layout of the building involving consideration of the location of rooms and walls openings such as doors and windows, the number of stories, etc. At this stage, site and foundation aspects should also be considered. Lay out and general design of the structural framing system with special attention to furnishing lateral resistance. Consideration of highly loaded and critical sections with provision of reinforcement as required. Studies has provided a good overview of structural action, mechanism of damage and modes of failure of buildings. From these studies, certain general principles have emerged: Structures should not be brittle or collapse suddenly. Rather, they should be tough, able to deflect or deform a considerable amount.Resisting elements, such as bracing or shear walls, must be provided evenly throughout the building, in both directions sidetoside, as well as top to bottom.All elements, such as walls and the roof, should be tied together so as to act as an integrated unit during earthquake shaking, transferring forces across connections and preventing separation.The building must be well connected to a good foundation and the earth. Wet, soft soils should be avoided, and the foundation must be well tied together, as well as tied to the wall.Care must be taken that all materials used are of good quality, and are protected from rain, sun, insects and other weakening actions, so that their strength lasts.Unreinforced earth and masonry have no reliable strength in tension and are brittle in compression. As a rule, they should be reinforced accordingly with steel or wood.

1. **METHODOLOGY**

The main building in the hills is a small complex with a house. Therefore, the focus of this paper is to study G + 4 and G + 7 buildings and understand their seismic response under cross-brace and diagonal brace, and compared to the last unbraded building. That is. A total of 6 models are created in STAAD pro and analyzed using the response spectrum method.

**BUILDING MODELS**

|  |  |  |
| --- | --- | --- |
| Building (Floors/Bracing) | G + 4 | G + 7 |
| Unbraced | Model – 1 | Model – 1 |
| Cross-bracing | Model – 2 | Model – 2 |
| Diagonal bracing | Model – 3 | Model - 3 |

**DESIGN PARAMETERS**

|  |  |
| --- | --- |
| Site condition | Jammu and Kashmir |
| Seismic zone | IV |
| Frame | SMRF |
| Importance factor | 1 |
| Codes | IS:456 , IS:800 , IS-1893 (Part -1), IS 875 (Part 1 - 4) |
| Soil condition | Hard |
| Software used | STAAD pro |
| Loads | Dead load, Live load , Wind load, Seismic load |
| Analysis method | Response spectrum method |

Shows the characteristics of the building frame members to be analyzed.

Analysis Method The analysis is based on the following assumptions.

1. The modulus of elasticity and Poisson's ratio are 25000 N / mm2 and 0.20, respectively.
2. Side effects PΔ, contraction and creep are not considered.
3. The soil membrane is rigid in its plane.
4. Axial deformation of the column is taken into account.
5. Each node in the frame has 6 degrees of freedom, 3 translations, and 3 rotations.
6. Torsion is considered according to IS: 1893 (I) –2002.
7. The material is homogeneous, isotropic and elastic

### Response Spectrum Analysis (RSA)

### Seismic analysis of all buildings is performed by the response spectrum method using IS: 1893 (I) –2002 [2]. This includes the effect of eccentricity (static + random). Other parameters used in seismic analysis are temperate seismic zone (IV), zone factor 0.24, importance factor 1.0, 5 ° mping and assuming a moment-sustaining framework common to all building configurations and heights. The response reduction factor is 3.0. Appropriate modes (at least 6) were considered for each construction case where the total modal mass of all modes is at least 99% of the total seismic mass. The bar force for each contribution mode with dynamic load was calculated and the modal response was combined using the CQC method. The following design spectra were used in the response spectrum analysis.

### Load combinations -

Load Combinations are taken as per **IS 1893** and are as follows:

In the limit state design of reinforced and pre-stressed concrete structures. Auto Load combination option of STAAD pro is used in this thesis.

**Analysis of results**

All buildings have been analyzed for seismic load with an effect of accidental eccentricity. The seismic force was applied in X direction and Z direction independently. Important results are presented in the subsequent sections.

**DISPLACMENT OF G + 4 & G +7 IN X AND Z DIRECTION**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| G + 4 CB DISPLACEMENT | G + 4 DB DISPLACEMENT | G + 4 DISPLACEMENT | G + 4 CB DISPLACEMENT | G + 4 DB DISPLACEMENT | G + 4 DISPLACEMENT |
| X mm | X mm | X mm | Z mm | Z mm | Z mm |
| 0.8 | 0.908 | 2.12 | 1.6 | 2.2 | 2.5 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| G + 7 CB DISPLACEMENT | G + 7 DB DISPLACEMENT | G + 7 DISPLACEMENT | G + 7 CB DISPLACEMENT | G + 7 DB DISPLACEMENT | G + 7 DISPLACEMENT |
| X mm | X mm | X mm | Z mm | Z mm | Z mm |
| 1.729 | 1.956 | 2.116 | 2.9 | 5.19 | 6.383 |

**Displacment of g+7 in x & z direction**

**DISPLACMENT IN X & Z DIRECTION**

**COMPARSION OF REACTION (FORCE) IN X AND Z DIRECTION**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| G+ 7 CB MAXI FORCES | G+ 7 DB MAXI FORCES | G+ 7 MAXI FORCES | G+ 7 CB MAXI FORCES | G+ 7 DB MAXI FORCES | G+ 7 MAXI FORCES |
| Fx kN | Fx kN | Fx kN | Fz kN | Fz kN | Fz kN |
| 887.425 | 1169.22 | 365.48 | 413.09 | 590.06 | 271.09 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| G+ 4 CB MAXI FORCES | G+ 4 DB MAXI FORCES | G+ 4 MAXI FORCES | G+ 4 CB MAXI FORCES | G+ 4 DB MAXI FORCES | G+ 4 MAXI FORCES |
| Fx kN | Fx kN | Fx kN | Fz kN | Fz kN | Fz kN |
| 356.001 | 438.044 | 240.487 | 148.45 | 215.277 | 189.309 |

**REACTION IN G + 4 BUILDIN**

**REACTION IN G + 7 BUILDING**

**REACTION COMPARISON IN X & Z DIRECTION**

**REACTION COMPARISON IN X & Z DIRECTION**

**COMPARSION OF REACTION MOMENT IN X AND Z DIRECTION**

**MOMENT TABLE FOR G +4**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| G+ 4 CB MAXI FORCES | G+ 4 DB MAXI FORCES | G+ 4 MAXI FORCES | G+ 4 CB MAXI FORCES | G+ 4 DB MAXI FORCES | G+ 4 MAXI FORCES |
| Mx kN-m | Mx kN-m | Mx kN-m | Mz kN-m | Mx kN-m | Mz kN-m |
| 32.118 | 63.66 | 48.335 | 23.85 | 48.33 | 67.731 |

MOMENT COMPARISON IN X & Z DIRECTION

MOMENT IN G + 7 BUILDING

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| G+ 7 CB MAXI FORCES | G+ 7 DB MAXI FORCES | G+ 7 MAXI FORCES | G+ 7 CB MAXI FORCES | G+ 7 DB MAXI FORCES | G+ 7 MAXI FORCES |
| Mx kN-m | Mx kN-m | Mx kN-m | Mz kN-m | Mx kN-m | Mz kN-m |
| 56.82 | 90.236 | 88.93 | 39.78 | 45.161 | 96.696 |

MOMENT COMPARISON IN X & Z DIRECTION

BASE SHEAR

**BASE SHEAR IN G + 4 & G+7 BUILDING**

|  |  |
| --- | --- |
| G+4 CB | 395.7 |
| G + 4 DB | 586.2 |
| G+4 | 513.92 |

|  |  |
| --- | --- |
| G+7 CB | 731.87 |
| G + 7 DB | 1269.82 |
| G+7 | 1208.35 |

**COMPARISON OF BASE SHEAR IN G + 4 & G+7 BUILDING**

1. **CONCLUSION**

After careful, computational analysis of all the different building models and bracing system it can be concluded that cross bracing system work more efficiently as it give minimum displacement, drift and member forces. Since cross bracing distribute more uniform forces through out the structure as well as provide more stiffness to the building frame hence very effective to the lateral stability of the building. Hence such bracing configuration may be very good for the Mid-rise building to be constructed in hilly area. Where as diagonal and unbraced system more or less perform very similar.

1. **REFERENCES**

[1] A.R. Chandrasekaran and D. S. Prakash Rao (2002), A seismic Design of Multi-storied RCC Buildings.

[2]A.S.Swathi, G.V. Rama Rao, R. A. B. Depaa “Seismic Performance Of Buildings On Sloping Grounds”. IJIREST volume 4, special issue 6, (May2015).

[3] Ajay Kumar Sreerama, Pradeep Kumar Ramancharla (2013), Earthquake behavior of reinforced concrete framed buildings on hill slopes. iternational Symposium on New Technologies for Urban Safety of Mega Cities in Asia (USMCA 2013) Report No: IIIT/TR/2013/-1.

[4] Birajdar.B.G,”Seismic analysis of buildings resting on sloping ground”, 13thWorld Conference on Earthquake Engineering, Vancouver, B.C., Canada, Paper No. 1472, 2004.

[5] Dr. R. B. Khadiranaikar1 and Arif Masali2 Seismic performance of buildings resting on sloping ground. IOSR J Mech Civ Eng (IOSR-JMCE) 11(3):12–19. [6]Dr. S. A. Halkude et al “Seismic Analysis of Buildings Resting on Sloping Ground With Varying Number of Bays and Hill Slopes” International Journal of Engineering Research and Technology ISSN:2278- 0181,Vol.2 Issue 12, December-2013.

[7]G.Suresh, and E.Arunakanth, “Seismic Analysis of Buildings Resting on Sloping Ground and Considering Bracing System”,International Journal of Engineering Research and Technology, Vol. 3,pp. 2278-0181, 2014.

[8]Likhitharadhya Y R, Praveen J V, Sanjith J, Ranjith A. “Seismic Analysis of Multi-Storey Building Resting On Flat Ground and Sloping Ground”. IJIRSET, (An ISO 3297: 2007 Certified Organization) Vol. 5, Issue 6, June 2016.

[9]Mohammed Umar Farooque Patel et al “A Performance study and seismic evaluation of RC frame buildings on sloping ground” IOSR Journal of Mechanical and Civil Engineering (IOSR-JMCE) e-ISSN: 2278-1684, p-ISSN: 2320-334X-, PP 51-58,2014.

[10]Mr.Tamboli Nikhil Vinod, Dr. Ajay Swarup. “study of seismic behaviour of multi-storied r.c.c. buildings resting on sloping ground and bracing system”. Vol-3 Issue-4 2017 IJARIIE-ISSN(O)-2395-4396.

[11] N. Jitendra Babu, K .Y.G.D Balaji “pushover analysis of unsymmetrical framed structures on sloping ground” International Journal of Civil, Structural, Environmental and Infrastructure Engineering Research and Development (IJCSEIERD) ISSN 2249- 6866 Vol. 2 Issue 4 Dec - 2012 45-54.

[12] Narayan Kalsulkar And Satish Rathod “ Seismic analysis of RCC building resting on sloping ground with varying number of bays and hill slopes”. IJCET journal volume 5.No.3 (june 2015) paper No 2063.

[13] Naveen Kumar S M, Vasipalli Vamsi Krishna Reddy, Supriya C L. “Analysis and Comparison of Step Back RC Frame Building on Sloping Strata and Plain Strata”. © 2017 IJRTI | Volume 2, Issue 9 | ISSN: 2456-3315.

[14]Paresh G. Mistry, Hemal J. Shah. “Seismic Analysis of Building on Sloping Ground Considering Bi-Directional Earthquake”. International Journal of Scientific Development and Research (IJSDR) [www.ijsdr.org.](http://www.ijsdr.org/) ISSN: 2455-2631 © April 2016 IJSDR | Volume 1, Issue 4.

[15]Prasad Ramesh Vaidya, “Seismic Analysis of Building with Shear Wall on Sloping Ground”. International Journal of Civil and Structural Engineering Research ISSN 2348-7607 (Online) Vol. 2, Issue 2, pp: (53-60), Month: October 2014 - March 2015, Available at: [www.researchpublish.com.](http://www.researchpublish.com/)

[16] Prashant D, Dr. Jagadish Kori G “ Seismic Response of one way slope RC frame building with soft storey” International Journal of Emerging Trends in Engineering and Development Issue 3, Vol.5 (September 2013).

[17] R. Nagarjuna, and S.B.Patil, “Lateral Stability of Multistorey Building on Sloping Ground”, International Research Journal of Engineering and Technology, Vol.02, pp.2395-0072, 2015.

[18] Ravikumar C M,\*, Babu Narayan K S “Effect of Irregular Configurations on Seismic Vulnerability of RC Buildings” Architecture Research2012,2(3):20-26DOI: 10.5923/j.arch.20120203.01.

[19]Ravindra Navale, Dr. Sandeep Hake, Pramod Kharmale. “analysis of unsymmetrical building resting on sloping ground by dividing in 2d frame”. (IRJET) e-ISSN: 2395- 0056 Volume: 04 Issue: 07 | July -2017 [www.irjet.net](http://www.irjet.net/) p- ISSN: 2395-0072.

[20] Rayyan-Ul-Hasan Siddiqui and , H. S. Vidyadhara “Seismic Analysis of Earthquake Resistant Multi Bay Multi Storeyed 3D – RC Frame” International Journal of Engineering Research & Technology (IJERT) ISSN: 2278- 0181 Vol. 2 Issue 10, October – 2013.

[21] Roser J. Robert, Ranjana M. Ghate (2016), “Seismic Analysis of Multistoried RCC Building on Sloping Ground”, International Journal For Research In Emerging Science And Technology, ISSN: 2349-7610, Vol. 03, Issue 12, pp. 40-45.

[22] S.K.Deshmukh, and F.I.Chavan Seismic Analysis of R.C.C. Building Resting on Sloping Ground”, International Journal of Pure and Applied Research in Engineering and Technology, Vol. 3, pp.119-133, 2015.

[23] S.M.Nagargoje and K.S.Sable," Seismic performance of multi-storeyed building on sloping ground", Elixir International Journal, 7 December 2012.

[24] Shivakumar Ganapati, Shivaraj Mangalgi. “pushover analysis of rc frame structure with floating column on sloping ground”. (IRJET) e-ISSN: 2395-0056 Volume: 04 Issue: 08 | Aug -2017 [www.irjet.net](http://www.irjet.net/) p-ISSN: 2395- 0072.

[25]Shivanand.B, H.S Vidyadhara “Design of 3D RC Frame on Sloping Ground” International Journal of Research in Engineering & Technology eISSN-2319-1163 pISSN:2312-7308 Volume 3 Issue:08 Aug 2014.

[26]Sujit kumar, Dr. Vivek garg, Dr. Abhay sharma (2014), “Effect Of Sloping Ground On Structural Performance Of Rcc Building Under Seismic Load”, ISSN: 2348-4098 VOLUME 2 ISSUE 6 AUGUST 2014 (VER [27] Y. Singh and Phani Gade “Seismic Behavior of Buildings Located on Slopes” - An Analytical Study and Some Observations from Sikkim Earthquake of September 18, 2011. 15th World Conference on Earthquake Engineering Journal 2012.

[28] Y. Singh, Phani Gade, D.H. Lang & E. Erduran (2014) : The linear and non-linear dynamic analysis shows that the storey at road level