**CFD Analysis and Thermal Enhancement of CuO Based Nano fluids**

**In a double pipe U -tube heat exchanger**

SHAILESH KUMAR YADAV1,

Research scholar, Department of Mechanical Engineering, Scope College of Engineering, Bhopal.

SURJEET SINGH RAJPOOT2,

Associate Professor, Department of Mechanical Engineering, Scope College of Engineering, Bhopal.

Dr. MUKESH KUMAR LALJI3

Principal - Part Time Diploma Course

I/c H.O.D. Architecture Department

S. V. Polytechnic College, Shyamla Hills, Bhopal (M.P.)

Department of Technical Education, Employment and Skill Development, M. P. Govt., Bhopal, Madhya Pradesh, India.

**Abstract**

Heat exchanger is used for heat transfer from one hot fluid to cold fluid. The performance of heat exchanger is analysed by of the heat transfer rate and heat transfer coefficient. The main objective of this research work is increased the performance of the heat exchanger by using Nano fluid. CFD analysis is performed for the estimation of heat transfer rate and heat transfer coefficient of Nano-fluid flow in a double pipe U-bend heat exchanger. The prototype of U-bend heat exchanger was developed using ANSYS 14.0 workbench. In this study Aluminium oxide (Al2O3,), Copper oxide (CuO), and Ethylene Glycol are used as a Nano fluids The volume fraction of Nano fluids are 0.2%, 0.3% and 0.4% were used in this analysis. The mass flow rate of hot fluid kept constant and the mass flow rate of Nano-fluids are varies from 0.154 kg/sec. The temperatures of Nano-fluids flow in a heat exchanger are kept at 343 K. The results revealed that as volume fraction are increased the heat transfer rate and heat transfer coefficient are increased, and Velocity and pressure are decreased. Based on the numerical results, the highest value of heat transfer coefficient is obtain from Al2O3 Nano-fluids with 0.02% volume fraction and highest heat transfer rate is CuO Nano fluid with 0.03% volume.

**Key words:** Nano fluid, Numerical analysis, Volume fraction, heat exchanger, heat transfer rate, enhancement of heat transfer.

**Introduction**

Heat exchanger is used for heat transfer from hot fluid to cold fluid. The performance of heat exchanger is analysed by of the heat transfer rate and heat transfer coefficient. The addition of Nano particles in the fluids is improves the performance of the heat exchanger and overall performance of the system. Nano fluids used in micro channels its latter properties considerably increased the heat transfer enhancement relative to “conventional” properties and heat transfer enhancement is comparable to the enhanced skin friction rise [1]. The nanoparticle suspension in three-phase system including the solid phase (nanoparticles), the liquid phase (fluid media), and the interfacial phase, which contributes significantly to the system properties because of its extremely high surface-to-volume ratio in Nano fluids [2]. MWCNT/water Nano fluids improves the heat transfer about 30% as compare to plain fluids and pressure drop enhanced about 11% [3]. Al2O3/water-based Nano-fluid improves the thermo-hydraulic performance of serpentine tube heat exchanger (STHX) [4]. Ferrous oxide Nano fluids improved the heat transfer and friction factor characteristics of a circular tube heat exchanger [5].Nano fluids used in micro channels its latter properties considerably increased the heat transfer enhancement relative to “conventional” properties and heat transfer enhancement is comparable to the enhanced skin friction rise [5]. Nano fluids improve both thermal and optical properties of current solar conversion systems. Direct solar thermal absorption collectors incorporating a Nano fluid offers the opportunity to achieve significant improvements in both optical and thermal performance. Since Nano fluids offer much greater heat absorbing and heat transfer properties compared to traditional working fluids [6]. Nano fluids increase the rate of heat transfer without affecting much the overall performance of the system, it is very useful in evaporators, air-conditioning equipment, thermal power plants, space vehicle, and automobile [7]. Nano fluid mixture with low concentration of solid particles are provided qualitative results regarding the heat transfer enhancement and provided heat transfer mechanisms [8]. Nano fluids showing the good result with Reynolds number of 20,000 and expansion ratio of 2.86, with methane [9]. Nano fluids improves the heat transfer of turbulent heat exchanger and separation flow in a symmetric expansion plane channel with the 5000 to 35,000 Reynolds number [10]. Standard *k*-*ε* model is very useful for calculated turbulent kinetic energy and velocity. This model presented the new trend for calculating the different parameter which is very useful for evaluating the performance of the turbulent flow heat exchanger [11]. Nano fluids have been used because of its higher thermal conductivity compared to traditional fluids. A new modified low-Reynolds number *k*-*ϵ* turbulence model showing the high wall heat transfer with Reynolds numbers ranging from 200 to 600 and different Nano fluids such as Cu, Ag, Al2O3, CuO, and TiO2 [12]. Al2O3, CuO, SiO2, and ZnO, with volume fraction that varied from 1% to 4% and the expansion ratio was 2, improves the heat transfer. Their results indicated that increasing Reynolds number and volume fraction augment Nusselt number; the highest Nusselt number value was associated with SiO2 [13]. Nano fluid flow and heat transfer over a backward-facing step, the results showed that the maximum heat transfer enhancement was about 26% and 36% for turbulent and laminar range, respectively, compared with pure water [14]. Al2O3-water Nano fluid flowing through a circular pipe showing the enhancement of heat transfer rate as compare to plain fluids [15]. The shape and size of Nano particles greatly affected the performance of Nano fluids. The smaller sizes of nano particles with spherical shape showing the higher heat transfer and enhanced the efficiency of the system [16]. The single phase dispersion model showed good performance compared to the other models [17]. Laminar TiO2-H2O Nano fluid flow in a horizontal circular pipe increase the heat transfer rate [18]. Al2O3– water Nano fluid flowing through a horizontal tube increase the heat transfer rate [19]. Cu-water Nano fluid flow in a circular tube under both the laminar and turbulent flow had increased the heat transfer coefficient [20]. The addition Al2O3 nano particles in the base fluids had helped to enhance the heat transfer rate. The maximum enhancement was observed to be 15% and 20% respectively at 3% under both the laminar and turbulent flow conditions [21]. Nano structured ceramic materials have used for as promising heat transfer fluid additives owing to their outstanding heat storage capacities [22]. Nano particles based nano fluids improves the heat transfer rate in both laminar and turbulent flow condition [23]. Copper oxide nano particles dispersed in ethylene glycol improves the heat transfer rate as compare to water mixture [24]. Al2O3 Nano fluid improves the heat transfer coefficient and reduced the friction factor [25].

**Methodology**

The CFD method follows the use of commercial software ANSYS FLUENT 14.0 for solving the problem. The solver in ANSYS-FLUENT used is a pressure correction based SIMPLE algorithm with 2ndorder upwind scheme for discretise the convective transport terms. The heat transfer coefficients are also obtained using CFD methods and compared with analytical values. After determining the important features of the problem following procedure is followed for solving the problem in which first of all we need to specify the solution method, and initialize the solution, then run the calculation. Initially create geometry model in the ANSYS workbench, as per the experimental setup design. Meshing was done on the geometry model by program controlled and sizing was done to get the required element size, nodes and smoothening. After getting the required size of element and meshing, naming selection was done to the domain before getting the results.

**Geometry and Modelling and boundary conditions**



Figure: -1 Schematic representation of

double pipe U-bend heat exchanger

Figure represents the schematic diagram of double pipe U-bend heat exchanger. The analysis is performed on a 2-pass double pipe heat exchanger with the inner diameter of inner pipe is 0.019 m & outer diameter of inner pipe is 0.025 m, similarly for annulus pipe, the inner diameter of outer pipe is 0.05 m & outer diameter of outer pipe is 0.056 m and the total length of heat exchanger is 2.36 m (2-pass). The mass flow rate of hot water kept constant over annulus section, with different temperatures and the mass flow rate of cold water constant. There is insulation for outer wall of annulus pipe with asbestos rope to minimize the heat losses.

**Meshing of geometry**

Structured meshing method in ANSYS WORKBENCH was used for the geometry. The element for meshing considered is hexahedral shape with number of elements of 876874 to 1240000. Naming selections were also done at required places.



Figure:-2Geometry modelling of 2-Pass

Double Pipe in ANSYS work bench

**Table:- 1** Grid test results & Final mesh

elements of 1124397 have been used for simulation

|  |  |  |
| --- | --- | --- |
| **No. of Elements** | **Cold water outlet temp (0C)** | **Hot water outlet temp (0C)** |
| 876874 | 31.458 | 53.970 |
| 895812 | 31.625 | 53.625 |
| 856253 | 30.256 | 44.325 |

**Boundary Conditions**

A Velocity inlet, uniform mass flow inlets and a constant inlet temperature were assigned at the channel inlet. At the exit, pressure was specified.

**Table:-2**  Boundary Conditions

|  |  |  |  |
| --- | --- | --- | --- |
| S.No. | Boundary Condition | Outer Pipe | Inner Pipe |
| 1 | Mass flow rate in inlet | 0.155 kg/s | 0.261 kg/s |
| 2 | Temperature | 342 K | 300 K |

**Thermo-Physical Properties of materials:**

Pure water is used as base fluid, and Nano particles of Al2O3, CuO and ethylene glycol fluid used as working fluid, the properties are shown in below.

**Table:-3** Thermo-Physical Properties of Nano particles

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Material** | **Thermal conductivity (W/m-k)** | **Specific heat (j/kg-k)** | **Density (kg/m3)** | **Viscosity (kg/m-s)** |
| Water | 0.605 | 4195 | 997.1 | 0.001003 |
| Al2O3 | 31.922 | 873.336 | 3950 | ---------- |
| Copper Oxide | 400 | 385 | 8933 | ---------- |
| Ethylene Glycol | 0.2580 | 837 | 1110 | ---------- |

**Results and discussion**

Three types of Nano fluids Aluminium Oxide (Al2O3), Copper Oxide (CuO) and Ethylene Glycol were used at three volume fractions in order to study the thermal performance of the heat exchanger the mass rate flow was 2Kg/s and the inlet temperature was 353K. For each Nano fluid, experiments were conducted for three volume fractions. Computational fluid dynamics (CFD) analysis of the heat exchanger by using all Nano fluids at three volume fractions (0.2, 0.3 and 0.4). Figure shows the velocity, pressure heat transfer rate, and heat transfer coefficients of different Nano fluids.

**Compression of Pressure and different nano fluid**

As can be seen the value of pressure increased dramatically when CuO was used at volume fraction 0.3 in comparisons with other Nano fluids. The lowest pressure was recorded when Ethylene Glycol was used at volume fraction 0.4.

Figure: -3 Pressure vs. Nano fluids

**Compression of Velocity and different Nano fluid**

As can be seen, the highest value was recorded within Ethylene Glycol at volume fraction 0.2 while the smallest value was documented within CuO fluid at volume fraction 0.4.This will effect of the movements of the fluids inside the heat exchanger.

Figure:-4 Velocity vs. Nano fluids

**Compression of Heat Transfer Coefficient values of different nano fluid**

The highest value was recorded when Al2O3 was used at volume fraction 0.2 while the smallest value was documented when Ethylene Glycol was used at volume fraction 0.4.

Figure: 5 Heat Transfer Coefficient vs. Nano fluids

**Compression of Heat Transfer Rate and different Nano fluid**

As can be seen, adding CuO nano particles to the base fluid increased heat transfer rate in comparison with other nano particles. It may be because the CuO Nano fluid has greatest thermal conductivity compared to other Nano fluid types.

Figure:-6Heat Transfer Rate vs. Nano fluids

**Conclusion**

Computational Fluid Dynamics (CFD) analysis was done on the heat exchanger for three types of Nano fluids (Al2O3, CuO and Ethylene Glycol) at three volume fractions (0.2, 0.3 and 0.4).

It can be concluded that,

* The value of pressure is more when CuO was used at volume fraction 0.3 in comparisons with other Nano fluids.
* The highest value of the heat exchanger outlet velocity was recorded within Ethylene Glycol at volume fraction 0.2.
* The highest values of the heat transfer coefficient was recorded when Al2O3 and CuO were used.
* The heat transfer rate was more when CuO nano particles were added to the base fluid in comparison with other nano particles.
* The high value of heat transfer rate for any cooling system indicated to better thermal performance of the cooling system.

It should be confirmed that increasing the heat transfer rate for any cooling system will indicate to better thermal performance of the cooling system. Overall, it can be said that CuO Nano fluid showed the best performance and Al2O3 Nano fluid was the second best in comparison with other Nano fluids.

**References**

[1] H. Togun, A. Tuqa, S.N. Kazi, A. Badarudin, M.K.A. Ariffin, H. Togun, A. Tuqa, S.N. Kazi, A. Badarudin, M.K.A. Ariffin, Heat transfer to laminar flow over a double backward-facing step, Int. J. Mech. Aerosp. Manuf. Ind. Sci. Eng. World Acad. Sci. Eng. Technol. 80 (2013) 117–139.

[2] T. Hussein, G. Ahmadi, TuqaAbdulrazzaq, Ahmed JassimShkarah, S.N. Kazi, A. Badarudin, et al., Thermal performance of nanofluid in ducts with double forward-facing steps, J. Taiwan Inst. Chem. Eng. 47 (2018) 28–42.

[3]. P.C. Mukesh Kumar, M. Chandrasekar “CFD analysis on heat and flow characteristics of double helically coiled tube heat exchanger handling MWCNT/water Nano fluids” Heliyon(ELSEVIER), Volume 5, pp.- e02030, 2019.

[4] [M.Awais](https://www.sciencedirect.com/science/article/abs/pii/S2451904920300421#!), [M.Saad](https://www.sciencedirect.com/science/article/abs/pii/S2451904920300421#!), [HamzaAyaz](https://www.sciencedirect.com/science/article/abs/pii/S2451904920300421#!), [M.M.Ehsan](https://www.sciencedirect.com/science/article/abs/pii/S2451904920300421#!), [Arafat.A.Bhuiyan](https://www.sciencedirect.com/science/article/abs/pii/S2451904920300421#!) “Computational Assessment of Nano-Particulate (Al2O3/Water) Utilization for Enhancement of Heat Transfer with varying straight section lengths in a Serpentine Tube Heat Exchanger” Thermal science and engineering progress (ELSEVIER) March 2020. (In press, journal pre proof).

[5].[G.Murali](https://www.sciencedirect.com/science/article/pii/S221478531931418X#!), [B.Nagendra](https://www.sciencedirect.com/science/article/pii/S221478531931418X#!), [J.Jaya](https://www.sciencedirect.com/science/article/pii/S221478531931418X#!), “CFD analysis on heat transfer and pressure drop characteristics of turbulent flow in a tube fitted with trapezoidal-cut twisted tape insert using Fe3O4 nano fluid. Materials today proceeding, [Volume 21,](https://www.sciencedirect.com/science/journal/22147853/21/part/P1) pp.- 313-319, 2020.

[6] M.R. Safaei, T. Hussein, K. Vafai, S.N. Kazi, A. Badarudin, Investigation of heat transfer enhancement in a forward-facing contracting channel using FMWCNT nanofluids, Numer. Heat Transfer, Part A Appl. 66 (2014) 1321–1361.

[7] T. Hussein, A. Tuqa, S.N. Kazi, H.K. Abdul Amir, B. Ahmed, M.K.A. A, et al., Numerical study of turbulent heat transfer in separated flow: review, Int. Rev. Mech. Eng. 7 (2013) 337–349.

[8] T. Hussein, A.J. Shkarah, S.N. Kazi, A. Badarudin, CFD simulation of heat transfer and turbulent fluid flow over a double forward-facing step, Math. Probl. Eng. 2013 (2013) 1–10.

[9] T. Hussein, T. Abdulrazzaq, S.N. Kazi, A. Badarudin, A.A.H. Kadhum, E. Sadeghinezhad, A review of studies on forced, natural and mixed heat transfer to fluid and nanofluid flow in an annular passage, Renew. Sust. Energ. Rev. 39 (2014) 835–856.

[10] L. Boelter, G. Young, H.W. Iversen, An Investigation of Aircraft Heaters XXVII—Distribution of Heat Transfer Rate in the Entrance Section of a Circular Tub. NACA-TN-1451, 1948.

[11] L. Khezzar, S.R.N. De Zilwa, J.H. Whitelaw, Combustion of premixed fuel and air downstream of a plane sudden-expansion, Exp. Fluids 27 (1999) 296–309.

[12] S. De Zilwa SR, J.H. Whitelaw Sivasegaram, Active control of isothermal and combusting flows in plane sudden-expansions, Proc. Transp. Phenom. Thermal Sci. Process Eng. (1997) 325–330.

[13] S.K. Park, T. Ota, An experimental approach to turbulent heat transfer using a symmetric expanded plane channel, J. Mech. Sci. Technol. 24 (2010) 857–863.

[14] C.C. Chieng, B.E. Launder, On the calculation of turbulent heat transport downstream from an abrupt pipe expansion, Numer. Heat Transfer 3 (1980) 189–207.

[15] B.T.F. Chung, S. Jia, A turbulent near-wall model on convective heat transfer from an abrupt expansion tube, Heat Mass Transf. 31 (1995) 33–40.

(16) W.D. Hsieh, K.C. Chang, Calculation of wall heat transfer in pipeexpansionturbulent flows, Int. J. Heat Mass Transf. 39 (1996) 3813–3822.

[17] D. Lee, J. Lee, H. Park, M. Kim, Experimental and numerical study of heat transfer downstream of an axisymmetric abrupt expansion and in a cavity of a circular tube, J. Mech. Sci. Technol. 25 (2011) 395–401.

(18) E. Abu-Nada, Application of nanofluids for heat transfer enhancement of separated flows encountered in a backward facing step, Int. J. Heat Fluid Flow 29 (2008) 242–249

[19] A.S. Kherbeet, H.A. Mohammed, B.H. Salman, The effect of nanofluids flow on mixed convection heat transfer over microscale backward-facing step, Int. J. Heat Mass Transf. 55 (2012) 5870–5881.

[20] H. Togun, M.R. Safaei, R. Sadri, S.N. Kazi, A. Badarudin, K. Hooman, et al., Numerical simulation of laminar to turbulent nanofluid flow and heat transfer over a backward-facing step, Appl. Math. Comput. 239 (2014) 153–170.

[21] B.C. Pak, Y.I. Cho, Hydrodynamic and heat transfer study of dispersed fluids with submicron metallic oxide nanoparticles, Experimental Heat transfer, 11 (1998) 150-170.

[22] Y. Xuan, Q. Li, Investigation on convective heat transfer and flow features of Nano fluids, Journal of Heat Transfer, 125 (2003) 151-155.

[23] Wen, D., & Ding, Y. (2004). Experimental investigation into convective heat transfer of Nano fluids at the entrance region under laminar flow conditions. International Journal of Heat and Mass Transfer, 47(24), 5181-5188.

[24] Namburu, P. K., Kulkarni, D. P., Misra, D., & Das, D. K. (2007). Viscosity of copper oxide nanoparticles dispersed in ethylene glycol and water mixture. Experimental Thermal and Fluid Science. 32(2), 397-402.

[25] Rao, G. S., Sharma, K. V., Chary, S. P., Bakar, R. A., Rahman, M. M., Kadirgama, K., & Noor, M. M. (2011). Experimental Study on heat transfer coefficient and friction factor of Al2O3 Nano fluid in a packed bed column. Journal of Mechanical Engineering and Sciences, 1, 1-15.