**Study and Analysis behaviour of reinforced concrete composite columns use the ANSYS software**

**Rohit Kumar1, Dr. Jyoti Yadav2**

1M.Tech Scholar, Dept. Of Civil Engineering, Sarvepalli Radhakrishnan University, Bhopal, M.P, India

2Assistant Professor, Dept. Of Civil Engineering, Sarvepalli Radhakrishnan University, Bhopal, M.P, India

**Abstract-**According to the requirements of advanced infrastructure, high-quality construction materials and innovative technologies are necessary. In recent years, the use of composite materials to reinforce concrete structures has increased. In this paper, numerous techniques for enhancing the performance of reinforced concrete columns using FRP composite material are examined. Using ANSYS, a linear analysis of a column specimen was conducted. The performed analysis will aid in determining the deformation of concrete columns reinforced with FRP bars.

**Keywords:- Fiber Reinforced Polymer (FRP), Linear Analysis, ANSYS**

**Introduction**

For many years, traditional reinforcing techniques in reinforced concrete columns have been used as a common practise among designers and builders. There has been much study, and designers can forecast how the columns will operate in the future. Fibre reinforced polymer (FRP) is used for structural reinforcement and rehabilitation. Because of their low weight, non-corrosiveness, high specific strength, specific stiffness, and ease of construction, FRP composites in the form of sheets, cables, rods, and plates have shown to be a future alternative to steel reinforcements [1,2]. AFRP, GFRP, and CFRP are typical forms of FRP employed in different research and real-world applications[3-5]. The goal of this study is to simulate and examine the behaviour of reinforced concrete columns strengthened with CFRP. The findings and observations reported in this research may help engineers anticipate the compressive strength of concrete columns made of CFRP.

**2. Objectives of the Study**

1. To examine the responses of steel-bar reinforced concrete columns to axial loads alone.

2. To investigate the behaviour of carbon fibre reinforced polymer-reinforced reinforced concrete columns under longitudinal and transverse compression under a pure axial load.

3. The structural behaviour of RCC and GFRP columns should be compared.

1. **Methodology**

In Fig. 1, the specifics of the testing columns were shown. Analysis was done on column specimens, each of which had a square cross-section with a length of 3000mm and a side of 400mm. Main steel and CFRP reinforcement for the examined columns was 8#16mm. The typical compressive strength of concrete columns is 30 N/mm2, and the transverse reinforcement (steel, GFRP) was about 6 mm stirrups spaced 250 mm apart.

****

Fig. 1:RCC columns

|  |  |  |  |
| --- | --- | --- | --- |
|  | Concrete | Steelreinforcement | CFRP |
| Unit Weight(N/mm3) | 2.40e-5 | 7.90e-5 | 1.60e-5 |
| Ultimate Compressive Strength(N/mm2) | 30 | NA | NA |
| TensileStrength(N/mm2) | 2.2 | 490 | 2070 |
| ElasticModulus(N/mm2) | 2.40e4 | 2e5 | 1.52e5 |
| Poisson ratio | 0.2 | 0.3 | 0.2 |

Table 1.Material Properties

The reinforcing ratios and kinds, concrete's typical compressive strength, ultimate load bearing capability, and other parametric studies are all considered in this inquiry.

|  |  |  |  |
| --- | --- | --- | --- |
| ColumnNo. | Reinforcement ratio(%) | Ultimate load on column(KN) | Remark |
| 1 | 0.8 | 2477 | Steel used asreinforcement |
| 2 | 0.8 | 4148 | CFRP used asreinforcemnt |

Table 2: Ultimate Load on column (KN)

1. **Results**

Table 3 compares deformations in columns reinforced with steel and CFRP and displays the analytical findings of deformations using ANSYS.

|  |  |  |  |
| --- | --- | --- | --- |
| ColumnNo | Reinforcementratio(%) | Deformation(mm) | Remark |
| 1 | 0.8 | 1.875 | Steel used asreinforcement |
| 2 | 0.8 | 2.785 | CFRP used asreinforcement |

Table 3: ANSYS Results for Deformation (Linear Analysis)

Equation of Elasticity for Composite Material is used to verify the values of deformations derived by ANSYS (In Linear Analysis). Table 4 show the verification of deformation in concrete columns reinforced with steel and CFRP.

|  |  |  |  |
| --- | --- | --- | --- |
| ColumnNo. | Reinforcementratio(%) | Deformation(mm) | Remark |
| 1 | 0.8 | 1.919 | Steel used asreinforcement |
| 2 | 0.8 | 3.220 | CFRP used asreinforcemnt |

Table 4: Validation for Deformation

|  |  |  |  |
| --- | --- | --- | --- |
| Column No. | Reinf ratio(%) | Costof Steel | Costof CFRP |
| 1 | 0.8 | 795 | 2835 |

Table 5: cost analysis & comparison

1. **Conclusions**
2. The values of deformation derived from the equation of elasticity for composite materials and the deformation findings from finite element analysis are in excellent agreement.
3. The ultimate load bearing capability of the column is greatly improved when made with CFRP.
4. Although CFRP is more expensive than steel reinforcement, it is ultimately more affordable because:

4. The CFRP has a stronger tensile strength, weighs 1/4 the amount of steel, is corrosion-free, and significantly lowers maintenance costs.

**References**

1. Benmokrane, B., El-Salakawy, E., El-Ragaby, A., and Lackey, T. [2006]. ―Designing and Testing of Concrete Bridge Decks Reinforced with Glass FRP Bars. ‖ Journal of Bridge Engineering, 11 (2): 217–229.
2. Demers, M., and Neale, K.W. [1999]. ―Confinement of Reinforced Concrete Columns with Fiber Reinforced Composite Sheets- an Experimental Study. ‖ Canadian Journal of Civil Engineering, 26, 226-241.
3. Teng, J.G., Chen, J.F., Smith, S.T., and Lam, L., [2002]. ―FRP Strengthened RC Structures.‖ John Wiley & Sons, New York, NY.
4. ACI Committee 440, (2006) “Guide for the design and construction of structural concrete reinforced with FRP bars,” ACI 440.1R-06, American Concrete Institute,

Farmington Hills, MI

1. Ching Chiaw Choo, Issam E. Harik, and Hans Gesund (2006) “Minimum Reinforcement Ratio for Fiber- Reinforced Polymer Reinforced Concrete Rectangular Columns” ACI Structural Journal/May-June, 460-466 pp
2. Ehab M. Lotfy, (2010) “Behaviour of reinforced concrete short columns with Fiber Reinforced polymers bars” International Journal of Civil and Structural Engineering Volume 1, No 3, pp 545-557