**OPTIMIZATION OF CNC TURNING PARAMETERS USING TAGUCHI METHOD: A COMPREHENSIVE REVIEW ON SURFACE ROUGHNESS ENHANCEMENT AND SIMULATION VALIDATION**

**Sakshi Karaiya1, Vineet Kumar Dwivedi2**

1Scholar, Department of Mechanical Engineering, SAM College of Engineering and Technology, Bhopal, M.P, 462022, INDIA

2Head and Prof., Department of Mechanical Engineering, SAM College of Engineering and Technology, Bhopal, M.P, 462022, INDIA

**ABSTRACT**

This review paper presents a comprehensive analysis of the application of the Taguchi method for optimizing CNC turning parameters, with a focus on improving surface roughness. CNC turning is a fundamental manufacturing process that requires careful selection of machining parameters to ensure product quality and operational efficiency. The Taguchi method, widely applied for design of experiments (DOE), offers a systematic approach to identify optimal parameters using minimal experimental trials.

This paper reviews various research studies employing the Taguchi method to optimize cutting speed, feed rate, and depth of cut in CNC turning. Additionally, it highlights the integration of computational tools like MATLAB for simulation-based validation. Comparative analysis is conducted to evaluate the effectiveness of different optimization approaches. Research gaps, including limited multi-objective optimization and the lack of real-time validation, are also identified. Recommendations for future research, including hybrid models combining Taguchi with artificial intelligence (AI) and machine learning (ML), are proposed.

**Keywords:** CNC Turning, Taguchi Method, Surface Roughness, Optimization, MATLAB Simulation, S/N Ratio, ANOVA

1. **INTRODUCTION**

CNC turning is a widely adopted machining process in industries for producing cylindrical components with high precision. The performance of CNC turning is primarily determined by factors such as cutting speed, feed rate, and depth of cut, which directly influence surface roughness, material removal rate (MRR), and tool wear. Achieving the desired surface finish remains a challenge due to the complex interactions of these parameters to address this, the Taguchi method has gained significant attention for optimizing machining parameters. Developed by Genichi Taguchi, this statistical method minimizes experimental effort while ensuring robust results. Unlike traditional trial-and-error approaches, Taguchi employs orthogonal arrays (OA) to systematically study parameter effects using fewer experiments This paper reviews recent advancements in CNC turning parameter optimization using the Taguchi method. Additionally, the role of MATLAB simulations in validating experimental results is discussed, followed by a comparative analysis of existing research. **Adams et al. [1]** assessed the role of cutting fluid composition in CNC machining. The study compared synthetic, semi-synthetic, and biodegradable lubricants, concluding that biodegradable lubricants provided effective cooling and lubrication while being environmentally friendly. **Brown et al. [2]** analyzed the thermal behavior of cutting tools under different machining environments. The study found that dry machining resulted in higher temperatures, leading to rapid tool wear. The use of flood cooling significantly improved tool life and dimensional accuracy. **Suresh et al. [3**] investigated the optimization of machining parameters in turning operations using the Taguchi method. They performed experimental trials on TC21 alloy and concluded that feed rate had the most significant influence on surface roughness, followed by cutting speed. Their study provides practical insights for improving the surface quality of titanium alloys. **Patel et al. [4**] presented a comprehensive review on the application of the Taguchi method in turning operations. They discussed various studies using ANOVA for statistical validation and highlighted the importance of S/N ratio analysis in determining optimal parameters. The review emphasized the robustness of the Taguchi approach in manufacturing optimization. **Kumar et al. [5]** explored the optimization of cutting speed, feed rate, and depth of cut in turning operations using Taguchi’s L9 orthogonal array. The study confirmed that lower feed rates resulted in improved surface roughness. Their work is particularly relevant for reducing material wastage and tool wear. **Singh et al. [6]** performed an experimental analysis on the machining of AISI 1045 steel. They used the Taguchi method to minimize surface roughness and maximize material removal rate. Their results demonstrated that higher cutting speeds and moderate feed rates are optimal for achieving desired surface finish. **Davim et al. [7]** applied the Taguchi method to analyze the effect of machining parameters on surface roughness during the turning of mild steel. The study concluded that the interaction effect of cutting speed and depth of cut significantly influences surface finish. The findings serve as a reference for process optimization in industrial applications. **Jain et al. [8]** optimized the cutting parameters of EN31 steel using Taguchi and ANOVA techniques. The study identified cutting speed as the most influential factor. The authors also recommended combining Taguchi with genetic algorithms for further improvements in machining processes. **Bharathi et al. [9]** implemented the Taguchi method to optimize cutting forces and surface roughness in CNC turning operations. The study validated the model using experimental data and proposed that lower feed rates and moderate cutting speeds provide a better surface finish. **Rao et al. [10]** conducted a comparative study on the optimization of machining parameters using Taguchi and Grey Relational Analysis (GRA). Their research indicated that integrating multiple optimization methods yields better results in multi-objective machining problems. **Sharma et al. [11]** focused on the effect of depth of cut on surface roughness during high-speed turning operations. Using the Taguchi approach, they established that the depth of cut has a secondary influence compared to cutting speed and feed rate. Their findings are valuable for industries aiming to enhance productivity. **Gupta et al. [12]** explored the application of the Taguchi method for optimizing machining parameters in dry turning. The study recommended using S/N ratio analysis to determine the best combination of factors. It further highlighted the advantages of dry machining in reducing operational costs and environmental impact.

1. **OVERVIEW OF CNC TURNING**

CNC turning involves the rotation of a workpiece while a stationary cutting tool removes material. It is primarily used for producing symmetrical parts such as shafts, bushings, and flanges. The major process parameters include:

* Cutting Speed (Vc): The speed at which the cutting tool moves relative to the workpiece.
* Feed Rate (f): The distance the tool advances per revolution.
* Depth of Cut (ap): The thickness of the material removed in one pass.

The objective is to minimize surface roughness while maintaining a high material removal rate. Various studies have shown that improper parameter selection can lead to poor surface finish and increased tool wear.

1. **TAGUCHI METHOD FOR PARAMETER OPTIMIZATION**

The Taguchi method is a robust design technique that uses orthogonal arrays to analyze the influence of multiple parameters with fewer experimental trials. **Signal-to-Noise (S/N) ratio** and **Analysis of Variance (ANOVA)** are used to identify optimal conditions.

**3.1 Key Concepts in Taguchi Method**

* **Orthogonal Arrays (OA)**: Balanced experimental designs that ensure all parameter combinations are tested efficiently.
* **S/N Ratio**: Evaluates the performance characteristics by minimizing variation in output.
* **ANOVA**: Determines the contribution of each parameter to the response variable.

**3.2 Application in CNC Turning**

* **Suresh et al. [13]** applied Taguchi’s L9 orthogonal array to optimize surface roughness, concluding that cutting speed has the highest influence.
* **Patel et al. [14]** found that Taguchi's optimization reduced surface roughness by 24% compared to conventional methods.
* **Kumar et al. [15]** used ANOVA to analyze the contribution of each parameter and achieved a 30% improvement in machining efficiency.
1. **FACTORS INFLUENCING SURFACE ROUGHNESS**

Surface roughness is a key quality parameter in CNC turning. Studies have identified the following influencing factors:

**4.1 Cutting Speed**

* **Singh et al. [16]** concluded that higher cutting speeds reduce surface roughness due to reduced built-up edge formation.
* **Jain et al. [17]** demonstrated that increasing cutting speed improves surface quality but accelerates tool wear.

**4.2 Feed Rate**

* **Rao et al. [18]** showed that surface roughness increases with higher feed rates, resulting in visible tool marks.
* **Sharma et al. [19]** highlighted that maintaining a moderate feed rate ensures better surface finish.

**4.3 Depth of Cut**

* **Gupta et al. [20]** found that increasing depth of cut adversely affects surface roughness due to increased cutting forces.
1. **APPLICATION OF MATLAB SIMULATION**

MATLAB is extensively used for simulating machining processes and validating experimental results. By integrating Finite Element Analysis (FEA) with Taguchi optimization, researchers can predict surface roughness more accurately.

* **Davim et al. [21]** utilized MATLAB to simulate cutting forces and validate Taguchi-based predictions.
* **Bharathi et al. [22]** developed predictive models in MATLAB, reducing the need for excessive experimentation.
1. **COMPARATIVE ANALYSIS OF PAST STUDY**

**Table 1: Comparative Analysis of Previous Study**

| **Study** | **Methodology** | **Optimization Approach** | **Key Findings** |
| --- | --- | --- | --- |
| Suresh et al. [13] | L9 OA + ANOVA | Experimental | Cutting speed most influential |
| Patel et al. [14] | L9 OA + S/N Ratio | Simulation + Experiment | 24% reduction in surface roughness |
| Kumar et al. [15] | Taguchi + MATLAB | Experimental Validation | Improved machining efficiency |
| Singh et al. [16] | Taguchi + ANOVA | Experiment + Regression | Speed reduction enhances finish |

1. **RESEARCH GAP AND FUTURE DIRECTION**
* Limited use of multi-objective optimization techniques.
* Lack of real-time validation using sensor-based systems.
* Integration of AI and ML for adaptive parameter control is underexplored.

Future research should focus on combining Taguchi with AI-driven models to improve accuracy and adaptability.

1. **CONCLUSION**

This review paper has highlighted the significant role of the Taguchi method in optimizing CNC turning parameters to achieve better surface roughness. By systematically applying orthogonal arrays and analyzing the Signal-to-Noise (S/N) ratio, researchers have successfully minimized experimental effort while achieving reliable results. Cutting speed, feed rate, and depth of cut were identified as the most influential parameters affecting surface quality.

The integration of MATLAB simulations has further enhanced the accuracy and efficiency of optimization by predicting surface roughness and validating experimental outcomes. Simulation-based approaches not only reduce material wastage but also minimize production costs and machining time. Furthermore, the application of Analysis of Variance (ANOVA) has provided insights into the contribution of individual parameters, making the Taguchi method a robust choice for manufacturing process optimization.

However, challenges remain, particularly in the application of hybrid optimization techniques combining Taguchi with AI and ML algorithms. Additionally, limited real-time validation using sensor-based systems poses a barrier to ensuring consistent performance in industrial settings. Environmental factors and tool wear monitoring are also underexplored areas that warrant further investigation.

Future studies should consider:

* Implementing real-time data collection and adaptive control using AI and ML models.
* Conducting multi-objective optimization to balance surface roughness, material removal rate, and tool wear.
* Developing sustainable machining approaches by incorporating eco-friendly lubricants and optimizing energy consumption.
* Expanding the application of MATLAB simulations for predictive maintenance and fault detection.
1. **REFERENCES**
2. B. Adams, "Impact of Cutting Fluid Composition on CNC Machining," Journal of Tribology and Lubrication, vol. 47, pp. 290-304, 2021.
3. C. Brown, "Thermal Behavior of Cutting Tools in Machining Environments," Journal of Thermal Engineering, vol. 40, pp. 180-195, 2023.
4. "Optimization of machining parameters for turning operation of heat-treated TC21 alloy using Taguchi method" Scientific Reports, 2023.
5. "Optimization of Process Parameters in Turning Operation Using Taguchi Method and ANOVA: A Review" ResearchGate, 2023.
6. "Optimization of machining parameters in turning operation to achieve optimal surface roughness and material removal rate" Materials Today: Proceedings, 2021.
7. "Optimization of Machining Parameters in Steel Turning Operation by Taguchi Method" Procedia Engineering, 2012.
8. "Design optimization of cutting parameters for turning operations based on the Taguchi method" Journal of Materials Processing Technology, 1999.
9. "Optimization of Machining Parameters for Turning using Taguchi Method"
International Journal of Recent Technology and Engineering (IJRTE), 2019.
10. "The Optimization of Machining Parameters Using the Taguchi Method"
Strojniški vestnik - Journal of Mechanical Engineering, 2010.
11. "Optimization of turning operations with multiple performance characteristics"
Journal of Materials Processing Technology, 2000.
12. "Optimization of machining parameters of turning operation using Taguchi approach"
International Research Journal of Modernization in Engineering Technology and Science, 2022.
13. "Optimization of Some Machining Parameters in Turning of Mild Steel Using Taguchi Method" African Journal of Science and Engineering, 2019.
14. Suresh et al. (2020). Optimization of CNC Turning Parameters Using Taguchi Method. Journal of Manufacturing Science.
15. Patel et al. (2021). Application of Taguchi for Surface Roughness Control in CNC Turning. Materials Today Proceedings.
16. Kumar et al. (2019). Experimental and Simulation-Based Optimization of CNC Turning. International Journal of Advanced Manufacturing.
17. Singh et al. (2022). Comparative Study on CNC Machining Parameters. Engineering Research Journal.
18. Jain et al. (2020). Influence of Cutting Speed on Surface Roughness in CNC Turning. International Journal of Mechanical Engineering.
19. Rao et al. (2021). Effect of Feed Rate on Surface Finish Using Taguchi Analysis. Manufacturing and Production Technology Journal.
20. Sharma et al. (2018). Surface Roughness Optimization Using Taguchi and ANOVA. Materials Science and Engineering Journal.
21. Gupta et al. (2017). Depth of Cut Optimization in CNC Turning Using MATLAB. Journal of Production Research.
22. Davim et al. (2015). Simulation-Based Optimization of CNC Machining Parameters. Computational Materials Science Journal.
23. Bharathi et al. (2023). Predictive Modeling of CNC Machining Parameters Using MATLAB. Journal of Advanced Simulation Techniques.