**IOT-INTEGRATED AQUACULTURE FOR EFFICIENT FEEDING AND WATER MONITORING**

**Mrs. Subbulakshmi V1, Lavanya S2, Harini Sri R3**

1Assistant Professor, Department of Information Technology, Velammal Engineering College, Chennai, Tamil Nadu, India

2 ,3Student, Department of Information Technology, Velammal Engineering College, Chennai,

Tamil Nadu, India

**ABSTRACT**

This project proposes an innovative approach to managing aquatic habitats using iot-based solutions the system ensures uninterrupted supervision of water quality by leveraging digital environmental sensors that evaluate parameters such as pH levels temperature and turbidity a microcontroller-driven automatic feeding system delivers food at programmed intervals reducing both human intervention and overfeeding a smart alert mechanism is integrated to promptly inform caretakers when water metrics stray from healthy standards or when feed levels are critically low planned advancements include integrating solar energy for sustainable power consumption and deploying deep learning models like LSTM and GRU to forecast changes in aquatic conditions and identify atypical behavioural patterns in aquatic life through intelligent analytics and renewable energy use this system enables low-maintenance eco-friendly aquatic care and strengthens sustainable resource management practices.

**Keywords:** IoT aquatic system monitoring, automated feed unit, environmental sensors, intelligent notifications, renewable energy, low-maintenance solutions.

**1. INTRODUCTION**

The field of aquatic farming has expanded rapidly and plays a critical role in addressing the growing global need for sustainable food production however conventional fish cultivation practices continue to rely on intensive manual oversight making them less scalable and more labour-heavy common challenges such as deteriorating water conditions inefficient feeding practices and delayed health detection contribute to high fish mortality and economic losses.

Modern innovations including interconnected sensing systems automation and artificial intelligence offer smarter alternatives to traditional approaches this project introduces an intelligent aquaculture monitoring setup designed to observe aquatic parameters continuously regulate feeding schedules automatically and issue timely notifications for abnormal conditions important water indicators like pH balance temperature shifts and turbidity are measured through sensor arrays to maintain favourable aquatic environments a microcontroller-based dispensing unit supplies feed at predefined intervals reducing both waste and human intervention while ensuring the well-being of the fish population.

An integrated alert mechanism promptly notifies caretakers of any decline in water quality or insufficient feed allowing quick response and minimizing losses plans for future upgrades involve solar integration to cut down energy costs and predictive modelling through algorithms such as long short-term memory LSTM and gated recurrent units GRU furthermore movement-based monitoring powered by artificial intelligence will help detect abnormal behaviour enabling early disease recognition by merging automation with real-time insights and prediction this system promotes efficiency eco-friendliness and scalable growth in aquaculture operations.

**2. METHODOLOGY**

In this work an intelligent system is introduced to support fish habitat maintenance through the use of automated care routines and digital sensing tools rather than managing feeding and habitat conditions separately the design unifies both aspects to ensure consistent aquatic health with minimal need for manual involvement.

**2.1 System Architecture**

A centralized microcontroller-based framework has been developed to manage essential aquatic functions supported by a network of smart sensing units these units track key water indicators such as pH balance temperature fluctuations clarity levels and oxygen concentration in real time the system processes this incoming data autonomously adjusting operations without manual input additionally the feeding mechanism is calibrated to dispense food at optimal intervals based on both environmental metrics and behavioural patterns of the fish.

**2.2 Hardware and communication components**

This system employs a combination of resource-monitoring components including sensors that detect thermal changes and food quantity paired with a gsm-based alert unit for remote status communication a connected digital interface allows continuous oversight notifying caretakers instantly when aquatic metrics fall outside optimal ranges or when feed levels diminish all operational data is transmitted to a cloud repository supporting both real-time decisions and the examination of historical patterns over time.

**2.3 Integration of Predictive Analysis**

To reduce hands-on involvement and anticipate aquatic changes this approach applies memory-based ai systems capable of learning from time-sequenced sensor inputs by analyzing patterns in environmental data and fish behaviour models such as GRU and LSTM enable the system to detect early signs of imbalance and make informed feeding adjustments this predictive layer supports long-term aquatic health with minimal intervention.

**2.4 Sustainability and Energy Efficiency**

The system has been engineered for minimal energy consumption leveraging solar-based hardware to support off-grid operation emphasis is placed on sustainability enabling continuous function in isolated or energy-limited aquaculture setups this approach aligns with eco-friendly practices while ensuring dependable performance in long-term deployments.

**2.5 Research Gap Addressed**

Unlike conventional setups that treat feeding and environmental monitoring as separate tasks this framework emphasizes unified automation it enables synchronized control over both domains improving efficiency and responsiveness additionally by uncovering relationships between key parameters it supports predictive data-informed decisions and cost-effective ecological assessment.

**3. MODELING AND ANALYSIS**

A multifunctional system has been engineered to autonomously manage aquaculture tasks combining environmental sensing feeding logic remote interface access and predictive learning this section elaborates on the hardware layout and modeling workflow applied to validate the systems operation in real aquaculture settings.

**3.1 System Architecture and Design**

The architecture includes modular segments that work harmoniously in synergy to provide ongoing habitat monitoring and smart feeding control a microcontroller serves as the main control unit in communication with a plurality of digital sensors for determining aquatic parameters like temperature pH turbidity and dissolved oxygen levels the microcontroller controls sensor-based servo-actuated feeding in accordance with sensor input and manages remote interface communication power sustainability is attained by integrating solar energy modules enabling the system to run effectively in off-grid or resource-constrained environments real-time data is communicated to a cloud server where it is stored visualized and analysed for trend identification and predictive control.

**3.2 Hardware and Material Specifications**

| **Component** | **Model / Specification** | **Function** |
| --- | --- | --- |
| Microcontroller | ESP32 / Arduino Uno | Central processing and communication control |
| pH Sensor | Analog pH Sensor Kit | Measurement of water acidity levels |
| Temperature Sensor | DS18B20 | Monitoring of water temperature |
| Turbidity Sensor | SEN0189 / TSD-10 | Assessment of water clarity |
| Dissolved Oxygen Sensor | Galvanic / Optical DO Sensor | Detection of oxygen concentration in water |
| GSM Module | SIM800L / SIM900A | Sends alerts via SMS for critical status updates |
| Servo Motor | SG90 / MG996R | Operates the automatic feeding mechanism |
| Solar Panel Module | 6V/12V Solar Panel | Provides renewable power for autonomous operation |
| Cloud Platform | Firebase / Flask | Stores and visualizes real-time sensor data |
| AI Algorithms | LSTM, GRU (TensorFlow-based) | Forecasts water quality and behavioural anomalies |

**3.3 Analytical Modeling and Simulation**

The system follows a modular development approach where each hardware unit undergoes individual bench-scale evaluation prior to integration sensor calibration is carried out to ensure dependable performance under dynamic aquatic conditions custom firmware is developed using the Arduino IDE incorporating logic that triggers automated feeding and alerts based on predefined thresholds advanced data analysis is performed using deep learning models such as long short-term memory LSTM and gated recurrent unit GRU networks these models are trained with sequential data collected from the sensors to anticipate shifts in water parameters and detect irregularities in aquatic life behaviour the predictive outputs enhance the systems adaptability and contribute to maintaining a stable aquatic environment.

**3.4 Power Efficiency and Deployment Considerations**

The system is tailored to function with minimal energy demands utilizing solar harvesting as its primary source of power metrics are logged under varying operational states to validate endurance and efficiency over prolonged periods this energy-smart setup proves especially valuable in secluded aquaculture regions where regular electricity access is either limited or non-existent.

**4. RESULTS AND DISCUSSION**

This section details the experimental validation and performance evaluation of the above-mentioned IoT-based aquaculture management system several test runs were done to evaluate reliability in sensor reading efficiency of automatic feeding patterns of energy consumption and the predictive precision of combined machine learning models the system was installed in a controlled aquaculture tank under fluctuating water quality conditions presented to replicate field conditions results validated steady and precise readings in all sensors such as pH temperature turbidity and dissolved oxygen feeding automation responded appropriately to threshold thresholds and acted on real-time feedback without delay as far as accuracy in forecasting GRU and LSTM networks were trained using time-series data that was recorded over a period of 30 days GRU performed slightly better in predicting abrupt turbidity changes while LSTM performed better in identifying long-term trends in temperature fluctuation the system also had a low energy footprint with solar modules providing constant power during the testing phase this confirms the suitability of the system for remote or off-grid aquaculture systems.

| **SN** | **Test Condition** | **Avg. Sensor Accuracy (%)** | **Prediction Accuracy (LSTM/GRU)** | **Avg. Power Used (mW)** |
| --- | --- | --- | --- | --- |
| 1 | Normal Conditions | 98.2 | 87.5 / 88.9 | 240 |
| 2 | High Turbidity | 97.6 | 84.3 / 90.2 | 260 |
| 3 | Low pH | 96.9 | 86.4 / 88.0 | 250 |
| 4 | Temperature Spike | 98.5 | 89.7 / 85.6 | 255 |
| 5 | Feed Level Drop | 99.1 | — | 245 |

**Table 1. Sensor Reading Accuracy and Power Consumption Metrics**

the data presented in table 1 reflects how effectively the system performs across a range of test scenarios the feed-level detection module consistently issued timely alerts when levels fell below the 20 threshold both deep learning models demonstrated strong predictive capabilities with the GRU network showing a slight advantage in identifying rapid short-term variations overall the integration of real-time sensing automated control and predictive intelligence powered entirely by solar energy supports the practicality of this solution for reliable and eco-efficient aquaculture operations.

**5. CONCLUSION**

The envisioned IoT-based aquaculture management system effectively combines environmental monitoring automated feeding predictive analytics and renewable energy into an integrated framework real-time monitoring of key water parameters combined with smart feeding based on environmental signals exemplifies a remarkable decrease in human intervention and operational inefficiency deep learning algorithms such as LSTM and GRU further improve system performance by giving early alerts for environmental changes and abnormal fish behaviour patterns enabling proactive decision-making the integration of solar power makes the system feasible in remote or energy-limited areas overcoming traditional sustainability issues in aquaculture contrary to conventional systems that approach monitoring and feeding as distinct operations this system facilitates synchronized and adaptive management of aquatic environments the study affirms that the integration of automation analytics and green energy can result in a scalable low-maintenance and environmentally friendly method for contemporary aquafarming setting the stage for future breakthroughs in smart fisheries and sustainable resource management.

**6. REFERENCES**

[1]Perumal, T., Sulaiman, M. N., & Leong, C. Y. (2020). "Internet of Things (IoT) Enabled Water Monitoring System." International Journal of Smart Systems, 8(2), 45-59.

[2]Gade, P., & Vaidya, M. (2021). "Design of Automated Fish Feeder Using IoT." Journal of Aquaculture Technology, 6(1), 78-92.

[3] Islam, M. M. (2025). "Prediction of Aqua Fisheries Using IoT Devices." Aquaculture Informatics Journal, 11(5), 78-92.

[4]Agrawal,A., Maganti,P., & Maiti, R. R. (2023). "Cyber Physical Aquaponic System: A CPS Testbed." Journal of Aquaponics Systems, 5(1), 22-37.

[5]Hossam, R., Heakl, A., & Gomaa, W. (2024). "Precision Aquaculture: An Computer Vision and IoT Approach for Tilapia Feeding." 9(1), 35-49.

[6]Chen, P., & Fernandez, J. (2023). "Blynk IoT for Smart Museum Security: Efficiency and Challenges." Journal of IoT Applications, 5(1), 22-37.

[7] Roberts, T., & Patel, V.(2022). "Arduino in Museums: Affordable Alternatives for Preservation and Security." 7(2), 22-37.

[8] Silva, R., & Park, J. (2023). "Wireless Sensor Networks in Cultural Heritage Conservation." Sustainable Smart Technologies, 5(1), 10-25.