## Secure Image Concealment through Pixel-Level Steganographic Embedding for Confidential Data Protection

# 1Shaik Mastan Basha, 2Gangolu Rajesh,3Raju Thommandru, 4Yamparala Nagendraiah

**1,2Asst. Professor, Dept. of ECE, Chalapathi Institute of Technology, Guntur, AP, India.**

**3Assoc. Professor, Dept. of ECE, Chalapathi Institute of Technology, Guntur, AP, India.**

**4Asst. Professor, Dept. of EEE, Chalapathi Institute of Technology, Guntur, AP, India.**

**ABSTRACT: Steganography plays a crucial role in modern information security systems by enabling the creation of concealed and secure communication channels between a sender and a receiver. This technique typically involves embedding a secret message within an image file. Recognizing the increasing need for secure communication, we propose a new algorithm designed to achieve the objectives of steganography effectively.This paper introduces a pixel-based image hiding method using steganography, where the pixels of a cover image serve as the medium for concealing secret text. The recipient can then apply a reverse extraction process to recover the original hidden message.The performance of this technique is evaluated using Peak Signal-to-Noise Ratio (PSNR) and capacity metrics. Experimental results demonstrate that our proposed method achieves higher data-hiding capacity compared to traditional approaches.**

**KEYWORDS: Steganography, Information Security, Pixel-Based Image Hiding, PSNR, Data Capacity.**

## INTRODUCTION

With rapid advancement in Multimedia technologies during the recent years, communication and information exchange have become much easier and faster but at the same time the issues related to data security and confidentiality have become a major concern of the time. Protection of transmitted digital images against illegal accessing, copying, modification, and distribution plays a crucial role in securing images transmissions over vulnerable networks [1]. Three basic security requirements must be met to have secured image transmission. These requirements are confidentiality, authenticity, and integrity. The confidentiality requirement means that only authorized users can have access to the image, whereas authenticity

verifies the owner of the transmitted image. Any modifications made to the image can be detected by enforcing the integrity requirement. Both Steganography and cryptography are two integral parts of information security.

Cryptography is the study of algorithms of sending messages in encrypted form (not understood) so that only the authorized recipients can decrypt message and read it. Cryptography system is classified into symmetric-key system and asymmetric- key system [2]. Symmetric-key system uses a single key that both the sender and the receiver have, and asymmetric-key system uses two different keys (a public- key and a private-key), where the public key is known to everyone and the private key is known to only the authorized recipient of messages uses.

Steganography is the process of hiding data under the image. In this process critical data is hidden into another piece of data which seems to be normal. It is done to keep the attacker unaware of the actual data [3]. This is implemented to avoid data leakage among unauthorized users of the system. The output is an image called stego-image that is similar to the cover media. This stego image is then sent to the receiver where the receiver retrieves the hidden message by applying the desteganography. A stego-key is used for embedding/encoding process to restrict decoding or extraction of the embedded data in cover media. The modern age steganography is usually implemented computationally, where multimedia files are used as cover media.

A good Steganographic mehods has three features, good hiding capacity, good imperceptibility and the last is robustness. The digital image Steganographic methods generally depends upon various image scrambling techniques in order to further improve the level of security of the hidden information. Image scrambling techniques scramble the pixels of an image in such a manner that the image becomes chaotic and indistinguishable. Hence, the message remains highly secured against unauthorised access.

Steganography can be split into two types, fragile and robust. In fragile steganography [4], information is embedded into a carrier called 'Cover' without being detected or retrieved by an attacker or unauthorized user. If the fragile data is modified then the secret data is destroyed as well without detection. On the other hand, robust steganography or sometimes known as digital watermarking aims to embed information into a cover while providing detection and protection capabilities if an attempt is made to destroy the cover.

Steganography techniques in the image can be divided into two categories, I) Steganography in the pixel domain (space domain), and II) in the transform domain such as frequency domain. In the case of pixel domain, the steganography operation is directly performed on the pixels. In transform domain steganography, the message embedding is performed in transformed image. The image is transformed from the space domain into a new domain such as frequency domain. This transforming can be done with different transforms such as Fourier and Wavelet transform. In our proposed system we have developed an algorithm which will be useful for pixel based data hiding and which satisfies the characteristics of steganography.

Remaining paper is organized as follows, Section introduces the Literature survey.

Section III presents described methodology. Section IV describes the results and finally paper concludes with Section V.

## LITERATURE SURVEY

Mohit Gupta, Praveen Kr. Tripathi et. al. [5], explained the steganography technique using BLINDHIDE algorithm along with its implementation and application. They proposed and implemented a method which hides secret data in color images by maintaining good visual quality and takes very less time in hiding and extraction of message. This method is based on third level two-dimensional discrete wavelet transform set by Haar wavelet. The main advantage is that there is no requirement of original image in extraction process which makes secret communication undetected by third party user or any steg analysis tools. They used Huffman coding for better imperceptibility result secret image. They used MATLAB R2014a for experimental activities.

Ankit Gambhir, Sibaram Khara, et. al. [6], explained the process that provides multilayer security by integrating cryptography with steganography. Fist they considered the message and performed the RSA encryption which resulted in a cipher text. They later hided the cipher text in audio using LSB audio steganography algorithm. Similarly, at receiver’s end, first cipher text is extracted from the audio cover then it is decrypted into message by using RSA decryption which combines both the features of steganography and cryptography and provides a higher level of security.

1. Qu and H. J. Kim, et. al. [7] presents Pixel-based pixel value ordering predictor for high-fidelity reversible data hiding. This technique combined sorting, prediction-error expansion and histogram shifting. Instead of scanning in a block-by- block manner, it predicted pixel in a pixel- by-pixel manner. In this way, pixel was

scanned in raster order and determined to be the current pixel. Other pixels in the same block of a rectangular region, one vertex of which is the current pixel are the context pixels. Obviously, this predictor provides more probability for obtaining prediction value than the aforementioned three category predictors. Holub, Vojtěch, Jessica Fridrich, and Tomáš Denemark, et. al. [8], the author defines a universal distortion function called universal wavelet relative distortion (UNIWARD) for steganography in the frequency space. The distortion is considered as the form of a sum of relative changes between the cover and embedded images that is represented in the transform domain and, it is computed in the wavelet domain as a sum of relative changes of coefficients in a directional filter bank decomposition of the cover image.

Rosziati Ibrahim, Teoh Suk Kuan, et. al. [9], explained an algorithm to hide data under image which uses binary codes and pixels inside an image. They used zipped file before it is converted to binary codes to maximize the storage of data inside the image. They developed a system called steganography imaging system which is then tested to see the viability of the proposed algorithm. Images stores various sizes of data and the Peak Signal-to-Noise Ratio (PSNR) is also captured for each of the images tested. Based on the PSNR value of each images, they stated that the stego image has a higher PSNR value.

D. M. Thodi and J. J. Rodriguez, et. al.

[10] describes Expansion embedding techniques for reversible watermarking. This new technique was combined with histogram shifting to embed data as an effective method. It well exploits the correlation inherent of the neighborhood pixels. The current pixel located on the block boundary. Context pixels cannot encircle the current pixel. Hence, only the preceding or subsequent partial pixels are effective for prediction. This type is

categorized to be half-enclosing prediction.

## III. PIXEL-BASED IMAGE HIDING USING STEGANOGRAPHY

This section describes Pixel based Image Hiding using Steganography. We have taken a text file which contains the secret text and an image file which will be act as cover image to hide the data. The process of image-based steganography is very simple. Images are composed of pixels which describes the content of image. Pixels are usually made up of colors. Every pixel is of combination of three colors red, green and blue. We kept the sole aim of maintaining the characteristics of image file.

**Embedding Process:** The process of embedding is performed in following steps:

* 1. Select a text file which contains the secret text.
  2. Select a cover image file of size M x N pixels. Create a sequence of pixels starting from 0,0 and so on and generate number of iterations for these sequences of pixels.
  3. Find the length of characters of the secret message.
  4. Run the loop for length of characters.

1. Firstly, the character is converted into 8-bit binary format using ASCII values.
2. Take first three set of pixels to encode. Each set has three values of red, green and blue each. So, there are total nine values. We have eight bits of the secret message character. So, if each color can be modified slightly, by setting the LSB to zero or one, these three pixels can store a byte with one value of color is left.
3. Taking the color values from left to right, change the pixel to even for 0 and odd for 1.
4. Previous step gives the new set of pixels. Save it.
5. Continue the process for each character.
   1. Replace the new set of pixels with set of original cover image pixels.
   2. Here is the secret message is embedded under the cover image.

Now, save the generated cover image. To share this cover image with authenticated user, use any secure way of data sharing by keeping in view that image should not be compressed or its dimension must not be changed. The best way of securely data sharing without losing its original dimension is email service but administrator can use any of the sharing medium.

Extracting process

Cover image

1. Save the byte of data in byte array,
2. Continue the process until the last bit of the last color of the last pixel that you read is 1.

c. Create the data set by collecting data from byte array.

d. Reveal the data to the user.

Image Recovery and Noise removal

Stego Image

Embedding process

Secret data

Replace the new set of pixels with original image pixels

Stego image

**Fig. 1: EMBEDDING PROCESS**

**Extraction Process:** For the data

to be

**Fig. 2: EXTRACTING PROCESS**

Based on the bits values in the embedded message, the pixel bits may be changed (increased or decreased). In the receiver side, the Extraction Process will be applied to the image, then the image pixels values are used together to retrieve the embedded message.

Save the new set of pixels

Take three set of pixels of RGB from left to encode

## RESULT ANALYSIS

In this section, performance evaluation of the proposed method is performed on the collection of some famous images using two standard criteria of steganography.

extracted at the user side, we need the steganograted image file which is shared by the administrator. We also need the algorithm which is used for embedding the data under the cover image.

The process of extraction is performed as following.

1. Select the steganograted image.
2. Generate the sequences of pixels.
3. Run the loop for sequences of pixels.
4. Consider the first three set of pixels from left to right.
5. Extract the data byte from the set of pixels by left shifting the pixels.

Examples of the images are shown in Fig

3. Following are the parameters derived on comparing the steganograted image generated by our proposed method with steganograted image generated by Blind Hide steganography algorithm. Peak signal to noise ratio (PSNR) and Capacity are used parameters.

Peak Signal to Noise Ratio (PSNR) expresses the similarity between the image before and after the steganography. The stego image should be similar to the

original (cover) image and their PSNR is calculated using below formula:

**PSNR**

100

50

PIH-S

BH-S

0

PIH-S

BH-S

B2

PSNR = 10. log10 (MSE) … . . (1)

M N

1

MSE(i1, i2) =

∑ ∑ [i1(x, y) − i2(x, y)]2 … . . (2)

NM

x=1 y=1

Where, B is the maximum fluctuation in the input image.



**Fig. 3: SAMPLES OF COVER IMAGES**

**Steganography capacity:** The steganography capacity expresses the amount of data that can be hidden per pixel and is calculated in bits per pixel unit. In order to evaluate this criterion, the maximum amount of the message bits that can be embedded in the image, with different compression quality, are calculated and their mean is considered as capacity.

Comparative analysis of Pixel based Image Hiding using Steganography (PIH-S) with steganograted image generated by Blind Hide steganography (BH-S) algorithm is represented in below Table 1.

**Table 1: COMPARATIVE ANALYSIS**

|  |  |  |
| --- | --- | --- |
| **Method used** | **PSNR** | **Capacity (considered for fox image)** |
| PIH-S | 65 | 57615 bits |
| BH-S | 54 | 56942 bits |

**Fig. 4: PSNR ANALYSIS**

**Capacity**

58000

57500

57000

56500

PIH-S

BH-S

PIH-S BH-S

**Fig. 5: CAPACITY ANALYSIS**

The result indicates that the Pixel based Image Hiding using Steganography method keeps high performance than Blind Hide steganography (BH-S) algorithm while increasing the embedded message volume.

## CONCLUSION

This paper discusses a pixel-based image hiding technique using steganography. The primary objective of steganography is to establish a secure and confidential communication channel between the sender and receiver. The embedding process follows a predefined replacement table, where pixel values are adjusted (either increased or decreased) based on the bit values of the hidden message.To assess the effectiveness of the proposed method, Peak Signal-to-Noise Ratio (PSNR) and the maximum data-hiding capacity are used as evaluation criteria. The results indicate that our approach can embed a larger volume of secret data while maintaining a stego image quality that closely resembles the original image.

## REFERENCES

1. Thommandru, R. (2024). Quantum Key Distribution for Securing 6G Networks: Shaping the Future of Mobile Communication. MJARET, 4(5), 16-20.
2. Thommandru, R., & Saravanakumar, R. (2022). Survey on MIMO Antenna for 5G Applications. Mathematical Statistician and Engineering Applications, 71(3), 2181-2191.
3. Reddy, V., Sk, K. B., Roja, D., Purimetla, N. R., Vellela, S. S., & Kumar, K. K. (2023, November). Detection of DDoS Attack in IoT Networks Using Sample elected RNN-ELM. In 2023 International Conference on Recent Advances in Science and Engineering Technology (ICRASET) (pp. 1-7). IEEE.
4. Sai Srinivas Vellela, M Venkateswara Rao, Srihari Varma Mantena, M V Jagannatha Reddy, Ramesh Vatambeti, Syed Ziaur Rahman, "Evaluation of Tennis Teaching Effect Using Optimized DL Model with Cloud Computing System", International Journal of Modern Education and Computer Science(IJMECS), Vol.16, No.2, pp. 16-28, 2024. DOI:10.5815/ijmecs.2024.02.02
5. Vullam, N., Roja, D., Rao, N., Vellela, S. S., Vuyyuru, L. R., & Kumar, K. K. (2023, November). Enhancing Intrusion Detection Systems for Secure ECommerce Communication Networks. In 2023 International Conference on the Confluence of Advancements in Robotics, Vision and Interdisciplinary Technology Management (IC-RVITM) (pp. 1-7). IEEE.
6. Vullam, N., Roja, D., Rao, N., Vellela, S. S., Vuyyuru, L. R., & Kumar, K. K. (2023, December). An Enhancing Network Security: A Stacked Ensemble Intrusion Detection System for Effective Threat Mitigation. In 2023 3rd International Conference on Innovative Mechanisms for Industry Applications (ICIMIA) (pp. 1314-1321). IEEE.
7. Basha, S. K., Purimetla, N. R., Roja, D., Vullam, N., Dalavai, L., & Vellela, S. S. (2023, December). A Cloud-based Auto-Scaling System for Virtual Resources to Back Ubiquitous, Mobile, Real-Time Healthcare Applications. In 2023 3rd International Conference on Innovative Mechanisms for Industry Applications (ICIMIA) (pp. 1223-1230). IEEE.
8. Rao, A. S., Dalavai, L., Tata, V., Vellela, S. S., Polanki, K., Kumar, K. K., & Andra, R. (2024, February). A Secured Cloud Architecture for Storing Image Data using Steganography. In 2024 2nd International Conference on Computer, Communication and Control (IC4) (pp. 1-6). IEEE.
9. Reddy, B. V., Sk, K. B., Polanki, K., Vellela, S. S., Dalavai, L., Vuyyuru, L. R., & Kumar, K. K. (2024, February). Smarter Way to Monitor and Detect Intrusions in Cloud Infrastructure using Sensor-Driven Edge Computing. In 2024 IEEE International Conference on Computing, Power and Communication Technologies (IC2PCT) (Vol. 5, pp. 918-922). IEEE.
10. Biyyapu, N., Veerapaneni, E. J., Surapaneni, P. P., Vellela, S. S., & Vatambeti, R. (2024). Designing a modified feature aggregation model with hybrid sampling techniques for network intrusion detection. Cluster Computing, 1-19.
11. Reddy, N. V. R. S., Chitteti, C., Yesupadam, S., Desanamukula, V. S., Vellela, S. S., & Bommagani, N. J. (2023). Enhanced speckle noise reduction in breast cancer ultrasound imagery using a hybrid deep learning model. Ingénierie des Systèmes d’Information, 28(4), 1063-1071.
12. Vellela, S. S., Vuyyuru, L. R., MalleswaraRaoPurimetla, N., Dalavai, L., & Rao, M. V. (2023, September). A Novel Approach to Optimize Prediction Method for Chronic Kidney Disease with the Help of Machine Learning Algorithm. In 2023 6th International Conference on Contemporary Computing and Informatics (IC3I) (Vol. 6, pp. 1677-1681). IEEE.
13. Davuluri, S., Kilaru, S., Boppana, V., Rao, M. V., Rao, K. N., & Vellela, S. S. (2023, September). A Novel Approach to Human Iris Recognition And Verification Framework Using Machine Learning Algorithm. In 2023 6th International Conference on Contemporary Computing and Informatics (IC3I) (Vol. 6, pp. 2447-2453). IEEE.
14. Vellela, S. S., Roja, D., Sowjanya, C., SK, K. B., Dalavai, L., & Kumar, K. K. (2023, September). Multi-Class Skin Diseases Classification with Color and Texture Features Using Convolution Neural Network. In 2023 6th International Conference on Contemporary Computing and Informatics (IC3I) (Vol. 6, pp. 1682-1687). IEEE.
15. Praveen, S. P., Nakka, R., Chokka, A., Thatha, V. N., Vellela, S. S., & Sirisha, U. (2023). A Novel Classification Approach for Grape Leaf Disease Detection Based on Different Attention Deep Learning Techniques. International Journal of Advanced Computer Science and Applications (IJACSA), 14(6).
16. Vellela, S. S., Reddy, V. L., Roja, D., Rao, G. R., Sk, K. B., & Kumar, K. K. (2023, August). A Cloud-Based Smart IoT Platform for Personalized Healthcare Data Gathering and Monitoring System. In 2023 3rd Asian Conference on Innovation in Technology (ASIANCON) (pp. 1-5). IEEE.
17. Vellela, S. S., & Balamanigandan, R. (2023). An intelligent sleep-awake energy management system for wireless sensor network. Peer-to-Peer Networking and Applications, 16(6), 2714-2731.
18. Vullam, N., Yakubreddy, K., Vellela, S. S., Sk, K. B., Reddy, V., & Priya, S. S. (2023, June). Prediction And Analysis Using A Hybrid Model For Stock Market. In 2023 3rd International Conference on Intelligent Technologies (CONIT) (pp. 1-5). IEEE.
19. Rao, K. N., Gandhi, B. R., Rao, M. V., Javvadi, S., Vellela, S. S., & Basha, S. K. (2023, June). Prediction and Classification of Alzheimer’s Disease using Machine Learning Techniques in 3D MR Images. In 2023 International Conference on Sustainable Computing and Smart Systems (ICSCSS) (pp. 85-90). IEEE.
20. Vellela, S. S., Vullum, N. R., Thommandru, R., Rao, T. S., Sowjanya, C., Roja, D., & Kumar, K. K. (2024, May). Improving Network Security Using Intelligent Ensemble Techniques: An Integrated System for Detecting and Managing Intrusions in Computer Networks. In 2024 International Conference on Advances in Modern Age Technologies for Health and Engineering Science (AMATHE) (pp. 1-7). IEEE.
21. Vullam, N., Vellela, S. S., Reddy, V., Rao, M. V., SK, K. B., & Roja, D. (2023, May). Multi-Agent Personalized Recommendation System in ECommerce based on User. In 2023 2nd International Conference on Applied Artificial Intelligence and Computing (ICAAIC) (pp. 1194-1199). IEEE.
22. Praveen, S. P., Sarala, P., Kumar, T. K. M., Manuri, S. G., Srinivas, V. S., & Swapna, D. (2022, November). An Adaptive Load Balancing Technique for Multi SDN Controllers. In 2022 International Conference on Augmented Intelligence and Sustainable Systems (ICAISS) (pp. 1403-1409). IEEE.
23. Vellela, S. S., & Balamanigandan, R. (2022, December). Design of Hybrid Authentication Protocol for High Secure Applications in Cloud Environments. In 2022 International Conference on Automation, Computing and Renewable Systems (ICACRS) (pp. 408-414). IEEE.
24. Vellela, S. S., & Balamanigandan, R. (2024). Optimized clustering routing framework to maintain the optimal energy status in the wsn mobile cloud environment. Multimedia Tools and Applications, 83(3), 7919-7938.
25. VenkateswaraRao, M., Vellela, S., Reddy, V., Vullam, N., Sk, K. B., & Roja, D. (2023, March). Credit Investigation and Comprehensive Risk Management System based Big Data Analytics in Commercial Banking. In 2023 9th International Conference on Advanced Computing and Communication Systems (ICACCS) (Vol. 1, pp. 2387-2391). IEEE.
26. Vellela, S. S., Reddy, B. V., Chaitanya, K. K., & Rao, M. V. (2023, January). An integrated approach to improve e-healthcare system using dynamic cloud computing platform. In 2023 5th International Conference on Smart Systems and Inventive Technology (ICSSIT) (pp. 776-782). IEEE.
27. Kumar, K. K., Rao, T. S., Vullam, N., Vellela, S. S., Jyosthna, B., Farjana, S., & Javvadi, S. (2024, March). An Exploration of Federated Learning for Privacy-Preserving Machine Learning. In 2024 5th International Conference on Innovative Trends in Information Technology (ICITIIT) (pp. 1-6). IEEE.
28. SrinivasVellela, S., Praveen, S. P., Roja, D., Krishna, A. R., Purimetla, N., Rao, T., & Kumar, K. K. (2024, April). Fusion-Infused Hypnocare: Unveiling Real-Time Instantaneous Heart Rates for Remote Diagnosis of Sleep Apnea. In 2024 International Conference on Knowledge Engineering and Communication Systems (ICKECS) (Vol. 1, pp. 1-5). IEEE.
29. Vellela, S. S., KOMMINENI, K. K., Rao, D. M. V., & Sk, K. B. (2024). An Identification of Plant Leaf Disease Detection Using Hybrid Ann and Knn. Sai Srinivas Vellela, Dr K Kiran Kumar, Dr. M Venkateswara Rao, Venkateswara Reddy B, Khader Basha Sk, Roja D, AN IDENTIFICATION OF PLANT LEAF DISEASE DETECTION USING HYBRID ANN AND KNN, Futuristic Trends in Artificial Intelligence, e.
30. Polasi, P. K., Vellela, S. S., Narayana, J. L., Simon, J., Kapileswar, N., Prabu, R. T., & Rashed, A. N. Z. (2024). Data rates transmission, operation performance speed and figure of merit signature for various quadurature light sources under spectral and thermal effects. Journal of Optics, 1-11.
31. Thommandru, R., Krishna, C. M., Suguna, N., Sathish, M., & Kiran, K. (2024, January). Millimetre Wave Self-Isolated MIMO Antenna with High Isolation and Radiation Efficiency. In 2024 2nd International Conference on Intelligent Data Communication Technologies and Internet of Things (IDCIoT) (pp. 191-196). IEEE.
32. Thommandru, R., Krishna, C. M., Suguna, N., Sathish, M., & Kiran, K. (2024, January). Millimetre Wave Self-Isolated MIMO Antenna with High Isolation and Radiation Efficiency. In 2024 2nd International Conference on Intelligent Data Communication Technologies and Internet of Things (IDCIoT) (pp. 191-196). IEEE.
33. Vellela, S. S., & Balamanigandan, R. (2024). Optimized clustering routing framework to maintain the optimal energy status in the wsn mobile cloud environment. *Multimedia Tools and Applications*, *83*(3), 7919-7938.
34. Vuyyuru, L. R., Purimetla, N. R., Reddy, K. Y., Vellela, S. S., Basha, S. K., & Vatambeti, R. (2024). Advancing automated street crime detection: a drone-based system integrating CNN models and enhanced feature selection techniques. *International Journal of Machine Learning and Cybernetics*, 1-23.
35. Krishna, C. V. M., Krishna, G. G., Vellela, S. S., Rao, M. V., Sivannarayana, G., & Javvadi, S. (2023, December). A Computational Data Science Based Detection of Road Traffic Anomalies. In 2023 Global Conference on Information Technologies and Communications (GCITC) (pp. 1-6). IEEE.
36. Vellela, S. S., & Balamanigandan, R. (2024). An efficient attack detection and prevention approach for secure WSN mobile cloud environment. Soft Computing, 1-15.
37. Saravanakumar, R., Raja, A., Narayan, P., Rajesh, G., Vinoth, M., & Thommandru, R. (2024, September). Dual-Band Performance Enhancement of Square Wheel Antennas with FR4 Substrate for Sub 7GHz Applications. In 2024 International Conference on Advances in Computing Research on Science Engineering and Technology (ACROSET) (pp. 1-7). IEEE.
38. Thommandru, R., Krishna, C. M., Suguna, N., Sathish, M., & Kiran, K. (2024, January). Millimetre Wave Self-Isolated MIMO Antenna with High Isolation and Radiation Efficiency. In 2024 2nd International Conference on Intelligent Data Communication Technologies and Internet of Things (IDCIoT) (pp. 191-196). IEEE.
39. Saravanakumar, R., Thommandru, R., Kumar, E. K., Al Ansari, M. S., Manage, P. S., & Muthuvel, S. K. (2024, April). Cross Scoop Fractal Antenna Design with Notch at 15 Degree for Emerging Applications at 5.2 GHz. In 2024 International Conference on Recent Advances in Electrical, Electronics, Ubiquitous Communication, and Computational Intelligence (RAEEUCCI) (pp. 1-7). IEEE.
40. Saravanakumar, R., Ponnapalli, V. P., Thommandru, R., Khatak, S., Manohara, H. T. P., & Thenmozhi, A. (2024, March). Analysis Circular Wave Guide Antenna for 5G Mid-Band Applications. In 2024 10th International Conference on Advanced Computing and Communication Systems (ICACCS) (Vol. 1, pp. 560-566). IEEE.
41. Thommandru, R., Krishna, C. M., Suguna, N., Sathish, M., & Kiran, K. (2024, January). Millimetre Wave Self-Isolated MIMO Antenna with High Isolation and Radiation Efficiency. In 2024 2nd International Conference on Intelligent Data Communication Technologies and Internet of Things (IDCIoT) (pp. 191-196). IEEE.
42. Thommandru, R., & Saravanakumar, R. (2022). Survey on MIMO Antenna for 5G Applications. Mathematical Statistician and Engineering Applications, 71(3), 2181-2191.
43. Madhuri, A., Jyothi, V. E., Praveen, S. P., Sindhura, S., Srinivas, V. S., & Kumar, D. L. S. (2024). A new multi-level semi-supervised learning approach for network intrusion detection system based on the ‘goa’. Journal of Interconnection Networks, 24(supp01), 2143047.
44. Thommandru, R., Kalyani, K., Rani, B. S., Karunakar, K., Sai, A. V., & Guptha, P. IoT Based Automatic Vehicle Accident Detection and Rescue System.
45. Madhuri, A., Praveen, S. P., Kumar, D. L. S., Sindhura, S., & Vellela, S. S. (2021). Challenges and issues of data analytics in emerging scenarios for big data, cloud and image mining. Annals of the Romanian Society for Cell Biology, 412-423.
46. Vellela, S. S., Balamanigandan, R., & Praveen, S. P. (2022). Strategic Survey on Security and Privacy Methods of Cloud Computing Environment. Journal of Next Generation Technology, 2(1).
47. Sk, K. B., Roja, D., Priya, S. S., Dalavi, L., Vellela, S. S., & Reddy, V. (2023, March). Coronary Heart Disease Prediction and Classification using Hybrid Machine Learning Algorithms. In 2023 International Conference on Innovative Data Communication Technologies and Application (ICIDCA) (pp. 1-7). IEEE.
48. Vellela, S. S., & Krishna, A. M. (2020). On Board Artificial Intelligence With Service Aggregation for Edge Computing in Industrial Applications. Journal of Critical Reviews, 7(07).
49. Kumar, E. R., Chandolu, S. B., Kumar, K. P. V., Rao, M. V., Muralidhar, V., Nagarjuna, K., & Vellela, S. S. (2023, November). UAVC: Unmanned Aerial Vehicle Communication Using a Coot Optimization-Based Energy Efficient Routing Protocol. In 2023 International Conference on Recent Advances in Science and Engineering Technology (ICRASET) (pp. 1-5). IEEE.
50. Vellela, S. S., Sowjanya, C., Vullam, N., Srinivas, B. R., Durga, M. L., Jyosthna, B., & Kumar, K. K. (2024, March). An Examination of Machine Learning Applications in the Field of Cybersecurity Approaches for Detecting and Mitigating Threats. In 2024 Third International Conference on Intelligent Techniques in Control, Optimization and Signal Processing (INCOS) (pp. 1-6). IEEE.